[SemImageFile]
Version=02-03
InstructName=TM3000
SerialNumber=113144-02
DataNumber=IFSC - USP8422
SampleName=
Format=JPG
ImageName=N781_P5.jpg
Directory=C:\Users\TM300\Documents\TM3000\Kelly Tasso\Filme aSi\micro femto incubacao\
SaveMode=2
Date=12/14/2022
Time=14:53:21
DateCheck=Yes
TimeCheck=Yes
NumberCheck=Yes
CommentCheck=Yes
DigitalZoom=No
Media=Drive_C
DataSize=1280x1100
DPI=191.81
PixelSize=66.21
SignalName=BSE COMPO
AcceleratingVoltage=15000 Volt
DecelerationVoltage=
Magnification=2000
WorkingDistance=5400 um
EmissionCurrent=42000 nA
FilamentCurrent=1750 mA
ObservationCondition=Analy
Brightness=2226
Contrast=4095
Rotation=12
LensMode=
PhotoSize=
Vacuum=Low
MicronMarker=30000
SubMagnification=
SubSignalName=
SpecimenBias=
Condencer2=1937
ScanSpeed=Slow3
CalibrationScanSpeed=
ColorMode=Grayscale
ColorPalette=
ScreenMode=
Comment=[]
KeyWord1=
KeyWord2=
Condition=Vacc=15.0kV   Mag=x2.0k   WD=5.40mm
DataDisplayCombine=
StageType=0
StagePositionX=0
StagePositionY=0
StagePositionR=
StagePositionZ=
StagePositionT=
